



Note: Some of the file names in this document’s screenshots have since been updated.









[Data]

comment=Raspberry Pi Data Share

path=/data

browseable=Yes

writeable=Yes

only guest=no

create mask=0777

directory mask=0777

public=no

[Web]

comment=Raspberry Pi Web Share

path=/var/www

browseable=Yes

writeable=Yes

only guest=no

create mask=0777

directory mask=0777

public=no

[Temp]

comment=Raspberry Pi RAM Share

path=/var/tmp

browseable=Yes

writeable=Yes

only guest=no

create mask=0777

directory mask=0777

public=no

**/etc/hostapd/hostapd.conf**

interface=wlan0

driver=rtl871xdrv

ssid=YOUR\_SSID

hw\_mode=g

channel=6

macaddr\_acl=0

auth\_algs=1

ignore\_broadcast\_ssid=0

wpa=2

wpa\_passphrase=YOUR\_PASSWORD

wpa\_key\_mgmt=WPA-PSK

wpa\_pairwise=TKIP

rsn\_pairwise=CCMP

**/etc/dhcp/dchpd.conf**

subnet 192.168.115.0 netmask 255.255.255.0 {

range 192.168.115.10 192.168.115.50;

option broadcast-address 192.168.115.255;

option routers 192.168.115.1;

default-lease-time 600;

max-lease-time 7200;

option domain-name "local";

option domain-name-servers 8.8.8.8, 8.8.4.4;

}